# Do not edit.
# Any changes will be lost on upgrade.
description=Standard Cisco Switch (template based)
radiusDisconnect=disconnect
acceptVlan= <<EOT
Tunnel-Medium-Type  = 6
Tunnel-Type = 13
Tunnel-Private-Group-Id = $vlan
EOT
acceptRole=Filter-Id = $role
reject=Reply-Message = This node is not allowed to use this service
disconnect= <<EOT
Calling-Station-Id = ${macToEUI48($mac)}
NAS-IP-Address = $disconnectIp
EOT
voip= <<EOT
Tunnel-Medium-Type  = 6
Tunnel-Type = 13
Cisco-AVPair = device-traffic-class=voice
EOT
