# Do not edit.
# Any changes will be lost on upgrade.
description=Meru Controller v2
radiusDisconnect=disconnect
acceptVlan=<<EOT
Tunnel-Medium-Type = 6
Tunnel-Type = 13
Tunnel-Private-Group-Id = $vlan
EOT
acceptRole=<<EOT
Filter-Id = $role
EOT
disconnect=<<EOT
Calling-Station-Id = $mac
EOT

