# Do not edit.
# Any changes will be lost on upgrade.
acceptVlan= <<EOT
Tunnel-Medium-Type = 6
Tunnel-Type = 13
Tunnel-Private-Group-Id = $vlan
EOT
voip=Egress-VLAN-Name = 1${switch._voiceRole}
acceptRole=
coa=
snmpDisconnect=enabled
disconnect=
description=Standard HP Switch (template based)
reject=Reply-Message = This node is not allowed to use this service
